PC Remote Design Doc

Suman Barick

# High Level Description

PCR or PC Remote will have 2 main components – The **“Web Controller (WC)”** in mobile device/browser and The **“Target Station (TS)”** in pc which is to be controlled. WC and TS will be connected via node socket.io connection. WC will feature a keyboard and mouse in the UI. Events will be sent to TS. TS will have a keyboard/mouse automation system via which it will trigger the same mouse and keyboard events on the target system.

# Detailed Design